

XXXXXX RF Test Report

|  |  |
| --- | --- |
| 作 者： |  |
| 日 期： | 2021-6-21 |

北京清微智能科技有限公司

版权所有 不得复制

Revision History

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Revision** | **Description** | **Author** |
| 2021-6-21 | V1.0 |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

table of Contents

[XXXXXX RF Test Report 1](#_Toc13301)

[Revision History 1](#_Toc4789)

[table of Contents 1](#_Toc27676)

[XXX RF Test Report 3](#_Toc25956)

[1 Overview 3](#_Toc30153)

[2 Test Configuration 3](#_Toc27088)

[2.1 DUT Information 3](#_Toc4168)

[2.2 Test Environment 3](#_Toc32429)

[3 Test summary 4](#_Toc4549)

[4 RF BT5 PHY BQB（BR and EDR）Test 5](#_Toc29332)

[4.1.1 RF/TRM/CA/BV-01-C [Output Power] 5](#_Toc8978)

[4.1.2 RF/TRM/CA/BV-02-C [Power Density] 5](#_Toc30021)

[4.1.3 RF/TRM/CA/BV-03-C [Power Control] 5](#_Toc32346)

[4.1.4 RF/TRM/CA/BV-04-C [TX Output Spectrum – Frequency Range] 6](#_Toc9213)

[4.1.5 RF/TRM/CA/BV-05-C [TX Output Spectrum – 20 dB Bandwidth] 7](#_Toc28831)

[4.1.6 RF/TRM/CA/BV-06-C [TX Output Spectrum – Adjacent Channel Power] 7](#_Toc4492)

[4.1.7 RF/TRM/CA/BV-07-C [Modulation Characteristics] 13](#_Toc7158)

[4.1.8 RF/TRM/CA/BV-08-C [Initial Carrier Frequency Tolerance] 14](#_Toc28690)

[4.1.9 RF/TRM/CA/BV-09-C [Carrier Frequency Drift] 14](#_Toc10465)

[4.1.10 RF/TRM/CA/BV-10-C [EDR Relative Transmit Power] 15](#_Toc29056)

[4.1.11 RF/TRM/CA/BV-11-C [EDR Carrier Frequency Stability and Modulation Accuracy] 16](#_Toc18228)

[4.1.12 RF/TRM/CA/BV-12-C [EDR Differential Phase Encoding] 17](#_Toc23893)

[4.1.13 RF/TRM/CA/BV-13-C [EDR In-band Spurious Emissions] 18](#_Toc9064)

[4.1.14 RF/TRM/CA/BV-14-C [Enhanced Power Control] 31](#_Toc3386)

[4.1.15 RF/RCV/CA/BV-01-C [Sensitivity – single slot packets] 32](#_Toc23376)

[4.1.16 RF/RCV/CA/BV-02-C [Sensitivity - multi-slot packets] 32](#_Toc20317)

[4.1.17 RF/RCV/CA/BV-03-C [C/I Performance] 32](#_Toc5499)

[4.1.18 RF/RCV/CA/BV-04-C [Blocking Performance] 34](#_Toc25787)

[4.1.19 RF/RCV/CA/BV-05-C [Intermodulation Performance] 35](#_Toc14557)

[4.1.20 RF/RCV/CA/BV-06-C [Maximum Input Level] 35](#_Toc17090)

[4.1.21 RF/RCV/CA/BV-07-C [EDR Sensitivity] 36](#_Toc28264)

[4.1.22 RF/RCV/CA/BV-08-C [EDR BER Floor Performance] 36](#_Toc15081)

[4.1.23 RF/RCV/CA/BV-09-C [EDR C/I Performance] 36](#_Toc9402)

[4.1.24 RF/RCV/CA/BV-10-C [EDR Maximum Input Level] 40](#_Toc57)

[5 RF BT5 PHY BQB（LE 1M）Test 41](#_Toc19992)

[5.1.1 RF/TRM-LE/CA/BV-01-C [Output power] 41](#_Toc469)

[5.1.2 RF/TRM-LE/CA/BV-03-C [In-band emissions, uncoded data at 1 Ms/s] 41](#_Toc4930)

[5.1.3 RF/TRM-LE/CA/BV-05-C [Modulation Characteristics, uncoded data at 1 Ms/s] 50](#_Toc2816)

[5.1.4 RF/TRM-LE/CA/BV-06-C [Carrier frequency offset and drift, uncoded data at 1Ms/s] 51](#_Toc18918)

[5.1.5 RF/RCV-LE/CA/BV-01-C [Receiver sensitivity, uncoded data at 1 Ms/s] 51](#_Toc23615)

[5.1.6 RF/RCV-LE/CA/BV-03-C [C/I and Receiver Selectivity Performance, uncoded data at 1 Ms/s] 52](#_Toc13251)

[5.1.7 RF/RCV-LE/CA/BV-04-C [Blocking Performance, uncoded data at 1 Ms/s] 53](#_Toc20093)

[5.1.8 RF/RCV-LE/CA/BV-05-C [Intermodulation Performance, uncoded data at 1 Ms/s] 53](#_Toc29617)

[5.1.9 RF/RCV-LE/CA/BV-06-C [Maximum input signal level, uncoded data at 1 Ms/s] 54](#_Toc22620)

[5.1.10 RF/RCV-LE/CA/BV-07-C [PER Report Integrity, uncoded data at 1 Ms/s] 54](#_Toc20529)

[6 RF BT5 PHY BQB（LE 2M）Test 54](#_Toc20258)

[6.1.1 RF/TRM-LE2M/CA/BV-01-C [Output power] 54](#_Toc22320)

[6.1.2 RF/TRM-LE2M/CA/BV-03-C [In-band emissions, uncoded data at 2 Ms/s] 54](#_Toc18391)

[6.1.3 RF/TRM-LE2M/CA/BV-05-C [Modulation Characteristics, uncoded data at 2 Ms/s] 63](#_Toc21788)

[6.1.4 RF/TRM-LE2M/CA/BV-06-C [Carrier frequency offset and drift, uncoded data at 2Ms/s] 64](#_Toc25235)

[6.1.5 RF/RCV-LE2M/CA/BV-01-C [Receiver sensitivity, uncoded data at 1 Ms/s] 65](#_Toc24966)

[6.1.6 RF/RCV-LE2M/CA/BV-03-C [C/I and Receiver Selectivity Performance, uncoded data at 2 Ms/s] 65](#_Toc22805)

[6.1.7 RF/RCV-LE2M/CA/BV-04-C [Blocking Performance, uncoded data at 2 Ms/s] 66](#_Toc5600)

[6.1.8 RF/RCV-LE2M/CA/BV-05-C [Intermodulation Performance, uncoded data at 2 Ms/s] 66](#_Toc13067)

[6.1.9 RF/RCV-LE2M/CA/BV-06-C [Maximum input signal level, uncoded data at 2 Ms/s] 67](#_Toc26391)

[6.1.10 RF/RCV-LE2M/CA/BV-07-C [PER Report Integrity, uncoded data at 2 Ms/s] 67](#_Toc21949)

[6.1.11 67](#_Toc8476)

XXX RF Test Report

# Overview

# Test Configuration

## DUT Information

## Test Environment

Equipment: CMW500 , shielding box , signal generator N5182B



Figure １ BR/EDR Hardware Connection Setup



Figure ２ LE Hardware Connection Setup

# Test summary

|  |  |  |
| --- | --- | --- |
| item | Test case | Pass/Fail |
| 1 | RF/TRM/CA/BV-01-C [Output Power] |  |
| 2 | RF/TRM/CA/BV-02-C [Power Density] |  |
| 3 | RF/TRM/CA/BV-03-C [Power Control] |  |
| 4 | RF/TRM/CA/BV-04-C [TX Output Spectrum – Frequency Range] |  |
| 5 | RF/TRM/CA/BV-05-C [TX Output Spectrum – 20 dB Bandwidth] |  |
| 6 | RF/TRM/CA/BV-06-C [TX Output Spectrum – Adjacent Channel Power] |  |
| 7 | RF/TRM/CA/BV-07-C [Modulation Characteristics] |  |
| 8 | RF/TRM/CA/BV-08-C [Initial Carrier Frequency Tolerance] |  |
| 9 | RF/TRM/CA/BV-09-C [Carrier Frequency Drift] |  |
| 10 | RF/TRM/CA/BV-10-C [EDR Relative Transmit Power] |  |
| 11 | RF/TRM/CA/BV-11-C [EDR Carrier Frequency Stability and Modulation Accuracy] |  |
| 12 | RF/TRM/CA/BV-12-C [EDR Differential Phase Encoding] |  |
| 13 | RF/TRM/CA/BV-13-C [EDR In-band Spurious Emissions] |  |
| 14 | RF/TRM/CA/BV-14-C [Enhanced Power Control] |  |
| 15 | RF/RCV/CA/BV-01-C [Sensitivity – single slot packets] |  |
| 16 | RF/RCV/CA/BV-02-C [Sensitivity - multi-slot packets] |  |
| 17 | RF/RCV/CA/BV-03-C [C/I Performance] |  |
| 18 | RF/RCV/CA/BV-04-C [Blocking Performance] |  |
| 19 | RF/RCV/CA/BV-05-C [Intermodulation Performance] |  |
| 20 | RF/RCV/CA/BV-06-C [Maximum Input Level] |  |
| 21 | RF/RCV/CA/BV-07-C [EDR Sensitivity] |  |
| 22 | RF/RCV/CA/BV-08-C [EDR BER Floor Performance] |  |
| 23 | RF/RCV/CA/BV-09-C [EDR C/I Performance] |  |
| 24 | RF/RCV/CA/BV-10-C [EDR Maximum Input Level] |  |
| 25 | RF/TRM-LE/CA/BV-01-C [Output power] |  |
| 26 | RF/TRM-LE/CA/BV-03-C [In-band emissions, uncoded data at 1 Ms/s] |  |
| 27 | RF/TRM-LE/CA/BV-05-C [Modulation Characteristics, uncoded data at 1 Ms/s] |  |
| 28 | RF/TRM-LE/CA/BV-06-C [Carrier frequency offset and drift, uncoded data at 1Ms/s] |  |
| 29 | RF/RCV-LE/CA/BV-01-C [Receiver sensitivity, uncoded data at 1 Ms/s] |  |
| 30 | RF/RCV-LE/CA/BV-03-C [C/I and Receiver Selectivity Performance, uncoded data at 1 Ms/s] |  |
| 31 | RF/RCV-LE/CA/BV-04-C [Blocking Performance, uncoded data at 1 Ms/s] |  |
| 32 | RF/RCV-LE/CA/BV-05-C [Intermodulation Performance, uncoded data at 1 Ms/s] |  |
| 33 | RF/RCV-LE/CA/BV-06-C [Maximum input signal level, uncoded data at 1 Ms/s] |  |
| 34 | RF/RCV-LE/CA/BV-07-C [PER Report Integrity, uncoded data at 1 Ms/s] |  |
| 35 | RF/TRM-LE2M/CA/BV-01-C [Output power] |  |
| 36 | RF/TRM-LE2M/CA/BV-03-C [In-band emissions, uncoded data at 2 Ms/s] |  |
| 37 | RF/TRM-LE2M/CA/BV-05-C [Modulation Characteristics, uncoded data at 2 Ms/s] |  |
| 38 | RF/TRM-LE2M/CA/BV-06-C [Carrier frequency offset and drift, uncoded data at 2Ms/s] |  |
| 39 | RF/RCV-LE2M/CA/BV-01-C [Receiver sensitivity, uncoded data at 2 Ms/s] |  |
| 40 | RF/RCV-LE2M/CA/BV-03-C [C/I and Receiver Selectivity Performance, uncoded data at 2 Ms/s] |  |
| 41 | RF/RCV-LE2M/CA/BV-04-C [Blocking Performance, uncoded data at 2 Ms/s] |  |
| 42 | RF/RCV-LE2M/CA/BV-05-C [Intermodulation Performance, uncoded data at 2 Ms/s] |  |
| 43 | RF/RCV-LE2M/CA/BV-06-C [Maximum input signal level, uncoded data at 2 Ms/s] |  |
| 44 | RF/RCV-LE2M/CA/BV-07-C [PER Report Integrity, uncoded data at 2 Ms/s] |  |

# RF BT5 PHY BQB（BR and EDR）Test

### RF/TRM/CA/BV-01-C [Output Power]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 1 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel:0 |  |  |  |  |  |
| Average Power | 0 | 20 |  | dBm |  |
| Peak Power |  | 23 |  | dBm |  |
| Channel:39 |  |  |  |  |  |
| Average Power | 0 | 20 |  | dBm |  |
| Peak Power |  | 23 |  | dBm |  |
| Channel:78 |  |  |  |  |  |
| Average Power | 0 | 20 |  | dBm |  |
| Peak Power |  | 23 |  | dBm |  |

### RF/TRM/CA/BV-02-C [Power Density]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 2 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Power Density:at 2420MHz |  | 20 |  | dBm |  |

### RF/TRM/CA/BV-03-C [Power Control]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 3 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel:0 |  |  |  |  |  |
| Power at Maximum | 0 | 20 |  | dBm |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power at Minimum |  | 4 |  | dBm |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power at Maximum |  |  |  | dBm |  |
| Channel:39 |  |  |  |  |  |
| Power at Maximum | 0 | 20 |  | dBm |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power at Minimum |  | 4 |  | dBm |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power at Maximum |  |  |  | dBm |  |
| Channel:78 |  |  |  |  |  |
| Power at Maximum | 0 | 20 |  | dBm |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power at Minimum |  | 4 |  | dBm |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power at Maximum |  |  |  | dBm |  |

### RF/TRM/CA/BV-04-C [TX Output Spectrum – Frequency Range]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 4 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| f(L):Channel 0 | 2400 |  |  | MHz |  |
| f(H):Channel 78 |  | 2483.5 |  | MHz |  |

### RF/TRM/CA/BV-05-C [TX Output Spectrum – 20 dB Bandwidth]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 5 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| f(L) |  |  |  | KHz |  |
| f(H) |  |  |  | KHz |  |
| f(H)-f(L) |  | 1000 |  | KHz |  |
| Channel : 39 |  |  |  |  |  |
| f(L) |  |  |  | KHz |  |
| f(H) |  |  |  | KHz |  |
| f(H)-f(L) |  |  |  | KHz |  |
| Channel : 78 |  |  |  |  |  |
| f(L) |  |  |  | KHz |  |
| f(H) |  |  |  | KHz |  |
| f(H)-f(L) |  |  |  | KHz |  |

### RF/TRM/CA/BV-06-C [TX Output Spectrum – Adjacent Channel Power]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 6 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel:3, Exceptions:0 |  |  |  |  |  |
| ACPower: 0 |  | -20 |  | dBm |  |
| ACPower: 1 |  | -20 |  | dBm |  |
| ACPower: 2 |  |  |  | dBm |  |
| ACPower: 3 |  |  |  | dBm |  |
| ACPower: 4 |  |  |  | dBm |  |
| ACPower: 5 |  | -20 |  | dBm |  |
| ACPower: 6 |  | -20 |  | dBm |  |
| ACPower: 7 |  | -40 |  | dBm |  |
| ACPower: 8 |  | -40 |  | dBm |  |
| ACPower: 9 |  | -40 |  | dBm |  |
| ACPower: 10 |  | -40 |  | dBm |  |
| ACPower: 11 |  | -40 |  | dBm |  |
| ACPower: 12 |  | -40 |  | dBm |  |
| ACPower: 13 |  | -40 |  | dBm |  |
| ACPower: 14 |  | -40 |  | dBm |  |
| ACPower: 15 |  | -40 |  | dBm |  |
| ACPower: 16 |  | -40 |  | dBm |  |
| ACPower: 17 |  | -40 |  | dBm |  |
| ACPower: 18 |  | -40 |  | dBm |  |
| ACPower: 19 |  | -40 |  | dBm |  |
| ACPower: 20 |  | -40 |  | dBm |  |
| ACPower: 21 |  | -40 |  | dBm |  |
| ACPower: 22 |  | -40 |  | dBm |  |
| ACPower: 23 |  | -40 |  | dBm |  |
| ACPower: 24 |  | -40 |  | dBm |  |
| ACPower: 25 |  | -40 |  | dBm |  |
| ACPower: 26 |  | -40 |  | dBm |  |
| ACPower: 27 |  | -40 |  | dBm |  |
| ACPower: 28 |  | -40 |  | dBm |  |
| ACPower: 29 |  | -40 |  | dBm |  |
| ACPower: 30 |  | -40 |  | dBm |  |
| ACPower: 31 |  | -40 |  | dBm |  |
| ACPower: 32 |  | -40 |  | dBm |  |
| ACPower: 33 |  | -40 |  | dBm |  |
| ACPower: 34 |  | -40 |  | dBm |  |
| ACPower: 35 |  | -40 |  | dBm |  |
| ACPower: 36 |  | -40 |  | dBm |  |
| ACPower: 37 |  | -40 |  | dBm |  |
| ACPower: 38 |  | -40 |  | dBm |  |
| ACPower: 39 |  | -40 |  | dBm |  |
| ACPower: 40 |  | -40 |  | dBm |  |
| ACPower: 41 |  | -40 |  | dBm |  |
| ACPower: 42 |  | -40 |  | dBm |  |
| ACPower: 43 |  | -40 |  | dBm |  |
| ACPower: 44 |  | -40 |  | dBm |  |
| ACPower: 45 |  | -40 |  | dBm |  |
| ACPower: 46 |  | -40 |  | dBm |  |
| ACPower: 47 |  | -40 |  | dBm |  |
| ACPower: 48 |  | -40 |  | dBm |  |
| ACPower: 49 |  | -40 |  | dBm |  |
| ACPower: 50 |  | -40 |  | dBm |  |
| ACPower: 51 |  | -40 |  | dBm |  |
| ACPower: 52 |  | -40 |  | dBm |  |
| ACPower: 53 |  | -40 |  | dBm |  |
| ACPower: 54 |  | -40 |  | dBm |  |
| ACPower: 55 |  | -40 |  | dBm |  |
| ACPower: 56 |  | -40 |  | dBm |  |
| ACPower: 57 |  | -40 |  | dBm |  |
| ACPower: 58 |  | -40 |  | dBm |  |
| ACPower: 59 |  | -40 |  | dBm |  |
| ACPower: 60 |  | -40 |  | dBm |  |
| ACPower: 61 |  | -40 |  | dBm |  |
| ACPower: 62 |  | -40 |  | dBm |  |
| ACPower: 63 |  | -40 |  | dBm |  |
| ACPower: 64 |  | -40 |  | dBm |  |
| ACPower: 65 |  | -40 |  | dBm |  |
| ACPower: 66 |  | -40 |  | dBm |  |
| ACPower: 67 |  | -40 |  | dBm |  |
| ACPower: 68 |  | -40 |  | dBm |  |
| ACPower: 69 |  | -40 |  | dBm |  |
| ACPower: 70 |  | -40 |  | dBm |  |
| ACPower: 71 |  | -40 |  | dBm |  |
| ACPower: 72 |  | -40 |  | dBm |  |
| ACPower: 73 |  | -40 |  | dBm |  |
| ACPower: 74 |  | -40 |  | dBm |  |
| ACPower: 75 |  | -40 |  | dBm |  |
| ACPower: 76 |  | -40 |  | dBm |  |
| ACPower: 77 |  | -40 |  | dBm |  |
| ACPower: 78 |  | -40 |  | dBm |  |
| Channel:39, Exceptions:0 |  |  |  |  |  |
| ACPower: 0 |  | -40 |  | dBm |  |
| ACPower: 1 |  | -40 |  | dBm |  |
| ACPower: 2 |  | -40 |  | dBm |  |
| ACPower: 3 |  | -40 |  | dBm |  |
| ACPower: 4 |  | -40 |  | dBm |  |
| ACPower: 5 |  | -40 |  | dBm |  |
| ACPower: 6 |  | -40 |  | dBm |  |
| ACPower: 7 |  | -40 |  | dBm |  |
| ACPower: 8 |  | -40 |  | dBm |  |
| ACPower: 9 |  | -40 |  | dBm |  |
| ACPower: 10 |  | -40 |  | dBm |  |
| ACPower: 11 |  | -40 |  | dBm |  |
| ACPower: 12 |  | -40 |  | dBm |  |
| ACPower: 13 |  | -40 |  | dBm |  |
| ACPower: 14 |  | -40 |  | dBm |  |
| ACPower: 15 |  | -40 |  | dBm |  |
| ACPower: 16 |  | -40 |  | dBm |  |
| ACPower: 17 |  | -40 |  | dBm |  |
| ACPower: 18 |  | -40 |  | dBm |  |
| ACPower: 19 |  | -40 |  | dBm |  |
| ACPower: 20 |  | -40 |  | dBm |  |
| ACPower: 21 |  | -40 |  | dBm |  |
| ACPower: 22 |  | -40 |  | dBm |  |
| ACPower: 23 |  | -40 |  | dBm |  |
| ACPower: 24 |  | -40 |  | dBm |  |
| ACPower: 25 |  | -40 |  | dBm |  |
| ACPower: 26 |  | -40 |  | dBm |  |
| ACPower: 27 |  | -40 |  | dBm |  |
| ACPower: 28 |  | -40 |  | dBm |  |
| ACPower: 29 |  | -40 |  | dBm |  |
| ACPower: 30 |  | -40 |  | dBm |  |
| ACPower: 31 |  | -40 |  | dBm |  |
| ACPower: 32 |  | -40 |  | dBm |  |
| ACPower: 33 |  | -40 |  | dBm |  |
| ACPower: 34 |  | -40 |  | dBm |  |
| ACPower: 35 |  | -40 |  | dBm |  |
| ACPower: 36 |  | -20 |  | dBm |  |
| ACPower: 37 |  | -20 |  | dBm |  |
| ACPower: 38 |  |  |  | dBm |  |
| ACPower: 39 |  |  |  | dBm |  |
| ACPower: 40 |  |  |  | dBm |  |
| ACPower: 41 |  | -20 |  | dBm |  |
| ACPower: 42 |  | -20 |  | dBm |  |
| ACPower: 43 |  | -40 |  | dBm |  |
| ACPower: 44 |  | -40 |  | dBm |  |
| ACPower: 45 |  | -40 |  | dBm |  |
| ACPower: 46 |  | -40 |  | dBm |  |
| ACPower: 47 |  | -40 |  | dBm |  |
| ACPower: 48 |  | -40 |  | dBm |  |
| ACPower: 49 |  | -40 |  | dBm |  |
| ACPower: 50 |  | -40 |  | dBm |  |
| ACPower: 51 |  | -40 |  | dBm |  |
| ACPower: 52 |  | -40 |  | dBm |  |
| ACPower: 53 |  | -40 |  | dBm |  |
| ACPower: 54 |  | -40 |  | dBm |  |
| ACPower: 55 |  | -40 |  | dBm |  |
| ACPower: 56 |  | -40 |  | dBm |  |
| ACPower: 57 |  | -40 |  | dBm |  |
| ACPower: 58 |  | -40 |  | dBm |  |
| ACPower: 59 |  | -40 |  | dBm |  |
| ACPower: 60 |  | -40 |  | dBm |  |
| ACPower: 61 |  | -40 |  | dBm |  |
| ACPower: 62 |  | -40 |  | dBm |  |
| ACPower: 63 |  | -40 |  | dBm |  |
| ACPower: 64 |  | -40 |  | dBm |  |
| ACPower: 65 |  | -40 |  | dBm |  |
| ACPower: 66 |  | -40 |  | dBm |  |
| ACPower: 67 |  | -40 |  | dBm |  |
| ACPower: 68 |  | -40 |  | dBm |  |
| ACPower: 69 |  | -40 |  | dBm |  |
| ACPower: 70 |  | -40 |  | dBm |  |
| ACPower: 71 |  | -40 |  | dBm |  |
| ACPower: 72 |  | -40 |  | dBm |  |
| ACPower: 73 |  | -40 |  | dBm |  |
| ACPower: 74 |  | -40 |  | dBm |  |
| ACPower: 75 |  | -40 |  | dBm |  |
| ACPower: 76 |  | -40 |  | dBm |  |
| ACPower: 77 |  | -40 |  | dBm |  |
| ACPower: 78 |  | -40 |  | dBm |  |
| Channel:75, Exceptions:0 |  |  |  |  |  |
| ACPower: 0 |  | -40 |  | dBm |  |
| ACPower: 1 |  | -40 |  | dBm |  |
| ACPower: 2 |  | -40 |  | dBm |  |
| ACPower: 3 |  | -40 |  | dBm |  |
| ACPower: 4 |  | -40 |  | dBm |  |
| ACPower: 5 |  | -40 |  | dBm |  |
| ACPower: 6 |  | -40 |  | dBm |  |
| ACPower: 7 |  | -40 |  | dBm |  |
| ACPower: 8 |  | -40 |  | dBm |  |
| ACPower: 9 |  | -40 |  | dBm |  |
| ACPower: 10 |  | -40 |  | dBm |  |
| ACPower: 11 |  | -40 |  | dBm |  |
| ACPower: 12 |  | -40 |  | dBm |  |
| ACPower: 13 |  | -40 |  | dBm |  |
| ACPower: 14 |  | -40 |  | dBm |  |
| ACPower: 15 |  | -40 |  | dBm |  |
| ACPower: 16 |  | -40 |  | dBm |  |
| ACPower: 17 |  | -40 |  | dBm |  |
| ACPower: 18 |  | -40 |  | dBm |  |
| ACPower: 19 |  | -40 |  | dBm |  |
| ACPower: 20 |  | -40 |  | dBm |  |
| ACPower: 21 |  | -40 |  | dBm |  |
| ACPower: 22 |  | -40 |  | dBm |  |
| ACPower: 23 |  | -40 |  | dBm |  |
| ACPower: 24 |  | -40 |  | dBm |  |
| ACPower: 25 |  | -40 |  | dBm |  |
| ACPower: 26 |  | -40 |  | dBm |  |
| ACPower: 27 |  | -40 |  | dBm |  |
| ACPower: 28 |  | -40 |  | dBm |  |
| ACPower: 29 |  | -40 |  | dBm |  |
| ACPower: 30 |  | -40 |  | dBm |  |
| ACPower: 31 |  | -40 |  | dBm |  |
| ACPower: 32 |  | -40 |  | dBm |  |
| ACPower: 33 |  | -40 |  | dBm |  |
| ACPower: 34 |  | -40 |  | dBm |  |
| ACPower: 35 |  | -40 |  | dBm |  |
| ACPower: 36 |  | -40 |  | dBm |  |
| ACPower: 37 |  | -40 |  | dBm |  |
| ACPower: 38 |  | -40 |  | dBm |  |
| ACPower: 39 |  | -40 |  | dBm |  |
| ACPower: 40 |  | -40 |  | dBm |  |
| ACPower: 41 |  | -40 |  | dBm |  |
| ACPower: 42 |  | -40 |  | dBm |  |
| ACPower: 43 |  | -40 |  | dBm |  |
| ACPower: 44 |  | -40 |  | dBm |  |
| ACPower: 45 |  | -40 |  | dBm |  |
| ACPower: 46 |  | -40 |  | dBm |  |
| ACPower: 47 |  | -40 |  | dBm |  |
| ACPower: 48 |  | -40 |  | dBm |  |
| ACPower: 49 |  | -40 |  | dBm |  |
| ACPower: 50 |  | -40 |  | dBm |  |
| ACPower: 51 |  | -40 |  | dBm |  |
| ACPower: 52 |  | -40 |  | dBm |  |
| ACPower: 53 |  | -40 |  | dBm |  |
| ACPower: 54 |  | -40 |  | dBm |  |
| ACPower: 55 |  | -40 |  | dBm |  |
| ACPower: 56 |  | -40 |  | dBm |  |
| ACPower: 57 |  | -40 |  | dBm |  |
| ACPower: 58 |  | -40 |  | dBm |  |
| ACPower: 59 |  | -40 |  | dBm |  |
| ACPower: 60 |  | -40 |  | dBm |  |
| ACPower: 61 |  | -40 |  | dBm |  |
| ACPower: 62 |  | -40 |  | dBm |  |
| ACPower: 63 |  | -40 |  | dBm |  |
| ACPower: 64 |  | -40 |  | dBm |  |
| ACPower: 65 |  | -40 |  | dBm |  |
| ACPower: 66 |  | -40 |  | dBm |  |
| ACPower: 67 |  | -40 |  | dBm |  |
| ACPower: 68 |  | -40 |  | dBm |  |
| ACPower: 69 |  | -40 |  | dBm |  |
| ACPower: 70 |  | -40 |  | dBm |  |
| ACPower: 71 |  | -40 |  | dBm |  |
| ACPower: 72 |  | -20 |  | dBm |  |
| ACPower: 73 |  | -20 |  | dBm |  |
| ACPower: 74 |  |  |  | dBm |  |
| ACPower: 75 |  |  |  | dBm |  |
| ACPower: 76 |  |  |  | dBm |  |
| ACPower: 77 |  | -20 |  | dBm |  |
| ACPower: 78 |  | -20 |  | dBm |  |

### RF/TRM/CA/BV-07-C [Modulation Characteristics]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 7 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Delta F1 Avg | 140 | 175 |  | KHz |  |
| Delta F2 99.9% | 115 |  |  | KHz |  |
| Delta F2 Avg / Delta F1 Avg | 0.8 |  |  |  |  |
| Channel : 39 |  |  |  |  |  |
| Delta F1 Avg | 140 | 175 |  | KHz |  |
| Delta F2 99.9% | 115 |  |  | KHz |  |
| Delta F2 Avg / Delta F1 Avg | 0.8 |  |  |  |  |
| Channel : 78 |  |  |  |  |  |
| Delta F1 Avg | 140 | 175 |  | KHz |  |
| Delta F2 99.9% | 115 |  |  | KHz |  |
| Delta F2 Avg / Delta F1 Avg | 0.8 |  |  |  |  |

### RF/TRM/CA/BV-08-C [Initial Carrier Frequency Tolerance]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 8 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Max. Frequency Tolerance | -75 | 75 |  | KHz |  |
| Channel : 39 |  |  |  |  |  |
| Max. Frequency Tolerance | -75 | 75 |  | KHz |  |
| Channel : 78 |  |  |  |  |  |
| Max. Frequency Tolerance | -75 | 75 |  | KHz |  |

### RF/TRM/CA/BV-09-C [Carrier Frequency Drift]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 9 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Max. Drift (DH1) | -25 | 25 |  | KHz |  |
| Max. Drift (DH3) | -40 | 40 |  | KHz |  |
| Max. Drift (DH5) | -40 | 40 |  | KHz |  |
| Max. Drift (DH1) ( / 50 us) | -20 | 20 |  | KHz |  |
| Max. Drift (DH3) ( / 50 us) | -20 | 20 |  | KHz |  |
| Max. Drift(DH5) ( / 50 us) | -20 | 20 |  | KHz |  |
| Channel : 39 |  |  |  |  |  |
| Max. Drift (DH1) | -25 | 25 |  | KHz |  |
| Max. Drift (DH3) | -40 | 40 |  | KHz |  |
| Max. Drift (DH5) | -40 | 40 |  | KHz |  |
| Max. Drift (DH1) ( / 50 us) | -20 | 20 |  | KHz |  |
| Max. Drift (DH3) ( / 50 us) | -20 | 20 |  | KHz |  |
| Max. Drift(DH5) ( / 50 us) | -20 | 20 |  | KHz |  |
| Channel : 78 |  |  |  |  |  |
| Max. Drift (DH1) | -25 | 25 |  | KHz |  |
| Max. Drift (DH3) | -40 | 40 |  | KHz |  |
| Max. Drift (DH5) | -40 | 40 |  | KHz |  |
| Max. Drift (DH1) ( / 50 us) | -20 | 20 |  | KHz |  |
| Max. Drift (DH3) ( / 50 us) | -20 | 20 |  | KHz |  |
| Max. Drift(DH5) ( / 50 us) | -20 | 20 |  | KHz |  |

### RF/TRM/CA/BV-10-C [EDR Relative Transmit Power]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 10 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Power DPSK - Power GFSK  2-DH5 | -4 | 1 |  | dB |  |
| Power GFSK  2-DH5 |  |  |  | dBm |  |
| Power DPSK  2-DH5 |  |  |  | dBm |  |
| Power DPSK - Power GFSK  3-DH5 | -4 | 1 |  | dB |  |
| Power GFSK  3-DH5 |  |  |  | dBm |  |
| Power DPSK  3-DH5 |  |  |  | dBm |  |
| Channel : 39 |  |  |  |  |  |
| Power DPSK - Power GFSK  2-DH5 | -4 | 1 |  | dB |  |
| Power GFSK  2-DH5 |  |  |  | dBm |  |
| Power DPSK  2-DH5 |  |  |  | dBm |  |
| Power DPSK - Power GFSK  3-DH5 | -4 | 1 |  | dB |  |
| Power GFSK  3-DH5 |  |  |  | dBm |  |
| Power DPSK  3-DH5 |  |  |  | dBm |  |
| Channel : 78 |  |  |  |  |  |
| Power DPSK - Power GFSK  2-DH5 | -4 | 1 |  | dB |  |
| Power GFSK  2-DH5 |  |  |  | dBm |  |
| Power DPSK  2-DH5 |  |  |  | dBm |  |
| Power DPSK - Power GFSK  3-DH5 | -4 | 1 |  | dB |  |
| Power GFSK  3-DH5 |  |  |  | dBm |  |
| Power DPSK  3-DH5 |  |  |  | dBm |  |

### RF/TRM/CA/BV-11-C [EDR Carrier Frequency Stability and Modulation Accuracy]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 11 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Omega i  2-DH5 | -75 | 75 |  | KHz |  |
| Omega i + Omega o  2-DH5 | -75 | 75 |  | KHz |  |
| Omega o  2-DH5 | -10 | 10 |  | KHz |  |
| DEVM RMS  2-DH5 |  | 20 |  | % |  |
| DEVM Peak  2-DH5 |  | 35 |  | % |  |
| DEVM 99%   1. DH5 |  | 30 |  | % |  |
| Omega i  3-DH5 | -75 | 75 |  | KHz |  |
| Omega i + Omega o  3-DH5 | -75 | 75 |  | KHz |  |
| Omega o  3-DH5 | -10 | 10 |  | KHz |  |
| DEVM RMS  3-DH5 |  | 13 |  | % |  |
| DEVM Peak  3-DH5 |  | 25 |  | % |  |
| DEVM 99%  3-DH5 |  | 20 |  | % |  |
| Channel : 39 |  |  |  |  |  |
| Omega i  2-DH5 | -75 | 75 |  | KHz |  |
| Omega i + Omega o  2-DH5 | -75 | 75 |  | KHz |  |
| Omega o  2-DH5 | -10 | 10 |  | KHz |  |
| DEVM RMS  2-DH5 |  | 20 |  | % |  |
| DEVM Peak  2-DH5 |  | 35 |  | % |  |
| DEVM 99%  2-DH5 |  | 30 |  | % |  |
| Omega i  3-DH5 | -75 | 75 |  | KHz |  |
| Omega i + Omega o  3-DH5 | -75 | 75 |  | KHz |  |
| Omega o  3-DH5 | -10 | 10 |  | KHz |  |
| DEVM RMS  3-DH5 |  | 13 |  | % |  |
| DEVM Peak  3-DH5 |  | 25 |  | % |  |
| DEVM 99%  3-DH5 |  | 20 |  | % |  |
| Channel : 78 |  |  |  |  |  |
| Omega i  2-DH5 | -75 | 75 |  | KHz |  |
| Omega i + Omega o  2-DH5 | -75 | 75 |  | KHz |  |
| Omega o  2-DH5 | -10 | 10 |  | KHz |  |
| DEVM RMS  2-DH5 |  | 20 |  | % |  |
| DEVM Peak  2-DH5 |  | 35 |  | % |  |
| DEVM 99%  2-DH5 |  | 30 |  | % |  |
| Omega i  3-DH5 | -75 | 75 |  | KHz |  |
| Omega i + Omega o  3-DH5 | -75 | 75 |  | KHz |  |
| Omega o  3-DH5 | -10 | 10 |  | KHz |  |
| DEVM RMS  3-DH5 |  | 13 |  | % |  |
| DEVM Peak  3-DH5 |  | 25 |  | % |  |
| DEVM 99%  3-DH5 |  | 20 |  | % |  |

### RF/TRM/CA/BV-12-C [EDR Differential Phase Encoding]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 12 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Packets with 0 errors  2-DH5 | 99 |  |  | % |  |
| Packets with 0 errors  3-DH5 | 99 |  |  | % |  |
| Channel : 39 |  |  |  |  |  |
| Packets with 0 errors  2-DH5 | 99 |  |  | % |  |
| Packets with 0 errors  3-DH5 | 99 |  |  | % |  |
| Channel : 78 |  |  |  |  |  |
| Packets with 0 errors  2-DH5 | 99 |  |  | % |  |
| Packets with 0 errors  3-DH5 | 99 |  |  | % |  |

### RF/TRM/CA/BV-13-C [EDR In-band Spurious Emissions]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 13 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Packet Type: 2-DH5 |  |  |  |  |  |
| Channel : 3,  Exceptions: 2 |  |  |  |  |  |
| ACPower: 0  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 1 |  | -20 |  | dBm |  |
| ACPower: 2,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 3,  Ptxref |  |  |  | dBm |  |
| ACPower: 4,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 5 |  | -20 |  | dBm |  |
| ACPower: 6,  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 7 |  | -40 |  | dBm |  |
| ACPower: 8 |  | -40 |  | dBm |  |
| ACPower: 9 |  | -40 |  | dBm |  |
| ACPower: 10 |  | -40 |  | dBm |  |
| ACPower: 11 |  | -40 |  | dBm |  |
| ACPower: 12 |  | -40 |  | dBm |  |
| ACPower: 13 |  | -40 |  | dBm |  |
| ACPower: 14 |  | -40 |  | dBm |  |
| ACPower: 15 |  | -40 |  | dBm |  |
| ACPower: 16 |  | -40 |  | dBm |  |
| ACPower: 17 |  | -40 |  | dBm |  |
| ACPower: 18 |  | -40 |  | dBm |  |
| ACPower: 19 |  | -40 |  | dBm |  |
| ACPower: 20 |  | -40 |  | dBm |  |
| ACPower: 21 |  | -40 |  | dBm |  |
| ACPower: 22 |  | -40 |  | dBm |  |
| ACPower: 23 |  | -40 |  | dBm |  |
| ACPower: 24 |  | -40 |  | dBm |  |
| ACPower: 25 |  | -40 |  | dBm |  |
| ACPower: 26 |  | -40 |  | dBm |  |
| ACPower: 27 |  | -40 |  | dBm |  |
| ACPower: 28 |  | -40 |  | dBm |  |
| ACPower: 29 |  | -40 |  | dBm |  |
| ACPower: 30 |  | -40 |  | dBm |  |
| ACPower: 31 |  | -40 |  | dBm |  |
| ACPower: 32 |  | -40 |  | dBm |  |
| ACPower: 33 |  | -40 |  | dBm |  |
| ACPower: 34 |  | -40 |  | dBm |  |
| ACPower: 35 |  | -40 |  | dBm |  |
| ACPower: 36 |  | -40 |  | dBm |  |
| ACPower: 37 |  | -40 |  | dBm |  |
| ACPower: 38 |  | -40 |  | dBm |  |
| ACPower: 39 |  | -40 |  | dBm |  |
| ACPower: 40 |  | -40 |  | dBm |  |
| ACPower: 41 |  | -40 |  | dBm |  |
| ACPower: 42 |  | -40 |  | dBm |  |
| ACPower: 43 |  | -40 |  | dBm |  |
| ACPower: 44 |  | -40 |  | dBm |  |
| ACPower: 45 |  | -40 |  | dBm |  |
| ACPower: 46 |  | -40 |  | dBm |  |
| ACPower: 47 |  | -40 |  | dBm |  |
| ACPower: 48 |  | -40 |  | dBm |  |
| ACPower: 49 |  | -40 |  | dBm |  |
| ACPower: 50 |  | -40 |  | dBm |  |
| ACPower: 51 |  | -40 |  | dBm |  |
| ACPower: 52 |  | -40 |  | dBm |  |
| ACPower: 53 |  | -40 |  | dBm |  |
| ACPower: 54 |  | -40 |  | dBm |  |
| ACPower: 55 |  | -40 |  | dBm |  |
| ACPower: 56 |  | -40 |  | dBm |  |
| ACPower: 57 |  | -40 |  | dBm |  |
| ACPower: 58 |  | -40 |  | dBm |  |
| ACPower: 59 |  | -40 |  | dBm |  |
| ACPower: 60 |  | -40 |  | dBm |  |
| ACPower: 61 |  | -40 |  | dBm |  |
| ACPower: 62 |  | -40 |  | dBm |  |
| ACPower: 63 |  | -40 |  | dBm |  |
| ACPower: 64 |  | -40 |  | dBm |  |
| ACPower: 65 |  | -40 |  | dBm |  |
| ACPower: 66 |  | -40 |  | dBm |  |
| ACPower: 67 |  | -40 |  | dBm |  |
| ACPower: 68 |  | -40 |  | dBm |  |
| ACPower: 69 |  | -40 |  | dBm |  |
| ACPower: 70 |  | -40 |  | dBm |  |
| ACPower: 71 |  | -40 |  | dBm |  |
| ACPower: 72 |  | -40 |  | dBm |  |
| ACPower: 73 |  | -40 |  | dBm |  |
| ACPower: 74 |  | -40 |  | dBm |  |
| ACPower: 75 |  | -40 |  | dBm |  |
| ACPower: 76 |  | -40 |  | dBm |  |
| ACPower: 77 |  | -40 |  | dBm |  |
| ACPower: 78 |  | -40 |  | dBm |  |
| Channel : 39,  Exceptions: 2 |  |  |  |  |  |
| ACPower: 0 |  | -40 |  | dBm |  |
| ACPower: 1 |  | -40 |  | dBm |  |
| ACPower: 2 |  | -40 |  | dBm |  |
| ACPower: 3 |  | -40 |  | dBm |  |
| ACPower: 4 |  | -40 |  | dBm |  |
| ACPower: 5 |  | -40 |  | dBm |  |
| ACPower: 6 |  | -40 |  | dBm |  |
| ACPower: 7 |  | -40 |  | dBm |  |
| ACPower: 8 |  | -40 |  | dBm |  |
| ACPower: 9 |  | -40 |  | dBm |  |
| ACPower: 10 |  | -40 |  | dBm |  |
| ACPower: 11 |  | -40 |  | dBm |  |
| ACPower: 12 |  | -40 |  | dBm |  |
| ACPower: 13 |  | -40 |  | dBm |  |
| ACPower: 14 |  | -40 |  | dBm |  |
| ACPower: 15 |  | -40 |  | dBm |  |
| ACPower: 16 |  | -40 |  | dBm |  |
| ACPower: 17 |  | -40 |  | dBm |  |
| ACPower: 18 |  | -40 |  | dBm |  |
| ACPower: 19 |  | -40 |  | dBm |  |
| ACPower: 20 |  | -40 |  | dBm |  |
| ACPower: 21 |  | -40 |  | dBm |  |
| ACPower: 22 |  | -40 |  | dBm |  |
| ACPower: 23 |  | -40 |  | dBm |  |
| ACPower: 24 |  | -40 |  | dBm |  |
| ACPower: 25 |  | -40 |  | dBm |  |
| ACPower: 26 |  | -40 |  | dBm |  |
| ACPower: 27 |  | -40 |  | dBm |  |
| ACPower: 28 |  | -40 |  | dBm |  |
| ACPower: 29 |  | -40 |  | dBm |  |
| ACPower: 30 |  | -40 |  | dBm |  |
| ACPower: 31 |  | -40 |  | dBm |  |
| ACPower: 32 |  | -40 |  | dBm |  |
| ACPower: 33 |  | -40 |  | dBm |  |
| ACPower: 34 |  | -40 |  | dBm |  |
| ACPower: 35 |  | -40 |  | dBm |  |
| ACPower: 36  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 37 |  | -20 |  | dBm |  |
| ACPower: 38,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 39,  Ptxref |  |  |  | dBm |  |
| ACPower: 40,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 41 |  | -20 |  | dBm |  |
| ACPower: 42,  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 43 |  | -40 |  | dBm |  |
| ACPower: 44 |  | -40 |  | dBm |  |
| ACPower: 45 |  | -40 |  | dBm |  |
| ACPower: 46 |  | -40 |  | dBm |  |
| ACPower: 47 |  | -40 |  | dBm |  |
| ACPower: 48 |  | -40 |  | dBm |  |
| ACPower: 49 |  | -40 |  | dBm |  |
| ACPower: 50 |  | -40 |  | dBm |  |
| ACPower: 51 |  | -40 |  | dBm |  |
| ACPower: 52 |  | -40 |  | dBm |  |
| ACPower: 53 |  | -40 |  | dBm |  |
| ACPower: 54 |  | -40 |  | dBm |  |
| ACPower: 55 |  | -40 |  | dBm |  |
| ACPower: 56 |  | -40 |  | dBm |  |
| ACPower: 57 |  | -40 |  | dBm |  |
| ACPower: 58 |  | -40 |  | dBm |  |
| ACPower: 59 |  | -40 |  | dBm |  |
| ACPower: 60 |  | -40 |  | dBm |  |
| ACPower: 61 |  | -40 |  | dBm |  |
| ACPower: 62 |  | -40 |  | dBm |  |
| ACPower: 63 |  | -40 |  | dBm |  |
| ACPower: 64 |  | -40 |  | dBm |  |
| ACPower: 65 |  | -40 |  | dBm |  |
| ACPower: 66 |  | -40 |  | dBm |  |
| ACPower: 67 |  | -40 |  | dBm |  |
| ACPower: 68 |  | -40 |  | dBm |  |
| ACPower: 69 |  | -40 |  | dBm |  |
| ACPower: 70 |  | -40 |  | dBm |  |
| ACPower: 71 |  | -40 |  | dBm |  |
| ACPower: 72 |  | -40 |  | dBm |  |
| ACPower: 73 |  | -40 |  | dBm |  |
| ACPower: 74 |  | -40 |  | dBm |  |
| ACPower: 75 |  | -40 |  | dBm |  |
| ACPower: 76 |  | -40 |  | dBm |  |
| ACPower: 77 |  | -40 |  | dBm |  |
| ACPower: 78 |  | -40 |  | dBm |  |
| Channel : 75,  Exceptions: 2 |  |  |  |  |  |
| ACPower: 0 |  | -40 |  | dBm |  |
| ACPower: 1 |  | -40 |  | dBm |  |
| ACPower: 2 |  | -40 |  | dBm |  |
| ACPower: 3 |  | -40 |  | dBm |  |
| ACPower: 4 |  | -40 |  | dBm |  |
| ACPower: 5 |  | -40 |  | dBm |  |
| ACPower: 6 |  | -40 |  | dBm |  |
| ACPower: 7 |  | -40 |  | dBm |  |
| ACPower: 8 |  | -40 |  | dBm |  |
| ACPower: 9 |  | -40 |  | dBm |  |
| ACPower: 10 |  | -40 |  | dBm |  |
| ACPower: 11 |  | -40 |  | dBm |  |
| ACPower: 12 |  | -40 |  | dBm |  |
| ACPower: 13 |  | -40 |  | dBm |  |
| ACPower: 14 |  | -40 |  | dBm |  |
| ACPower: 15 |  | -40 |  | dBm |  |
| ACPower: 16 |  | -40 |  | dBm |  |
| ACPower: 17 |  | -40 |  | dBm |  |
| ACPower: 18 |  | -40 |  | dBm |  |
| ACPower: 19 |  | -40 |  | dBm |  |
| ACPower: 20 |  | -40 |  | dBm |  |
| ACPower: 21 |  | -40 |  | dBm |  |
| ACPower: 22 |  | -40 |  | dBm |  |
| ACPower: 23 |  | -40 |  | dBm |  |
| ACPower: 24 |  | -40 |  | dBm |  |
| ACPower: 25 |  | -40 |  | dBm |  |
| ACPower: 26 |  | -40 |  | dBm |  |
| ACPower: 27 |  | -40 |  | dBm |  |
| ACPower: 28 |  | -40 |  | dBm |  |
| ACPower: 29 |  | -40 |  | dBm |  |
| ACPower: 30 |  | -40 |  | dBm |  |
| ACPower: 31 |  | -40 |  | dBm |  |
| ACPower: 32 |  | -40 |  | dBm |  |
| ACPower: 33 |  | -40 |  | dBm |  |
| ACPower: 34 |  | -40 |  | dBm |  |
| ACPower: 35 |  | -40 |  | dBm |  |
| ACPower: 36 |  | -40 |  | dBm |  |
| ACPower: 37 |  | -40 |  | dBm |  |
| ACPower: 38 |  | -40 |  | dBm |  |
| ACPower: 39 |  | -40 |  | dBm |  |
| ACPower: 40 |  | -40 |  | dBm |  |
| ACPower: 41 |  | -40 |  | dBm |  |
| ACPower: 42 |  | -40 |  | dBm |  |
| ACPower: 43 |  | -40 |  | dBm |  |
| ACPower: 44 |  | -40 |  | dBm |  |
| ACPower: 45 |  | -40 |  | dBm |  |
| ACPower: 46 |  | -40 |  | dBm |  |
| ACPower: 47 |  | -40 |  | dBm |  |
| ACPower: 48 |  | -40 |  | dBm |  |
| ACPower: 49 |  | -40 |  | dBm |  |
| ACPower: 50 |  | -40 |  | dBm |  |
| ACPower: 51 |  | -40 |  | dBm |  |
| ACPower: 52 |  | -40 |  | dBm |  |
| ACPower: 53 |  | -40 |  | dBm |  |
| ACPower: 54 |  | -40 |  | dBm |  |
| ACPower: 55 |  | -40 |  | dBm |  |
| ACPower: 56 |  | -40 |  | dBm |  |
| ACPower: 57 |  | -40 |  | dBm |  |
| ACPower: 58 |  | -40 |  | dBm |  |
| ACPower: 59 |  | -40 |  | dBm |  |
| ACPower: 60 |  | -40 |  | dBm |  |
| ACPower: 61 |  | -40 |  | dBm |  |
| ACPower: 62 |  | -40 |  | dBm |  |
| ACPower: 63 |  | -40 |  | dBm |  |
| ACPower: 64 |  | -40 |  | dBm |  |
| ACPower: 65 |  | -40 |  | dBm |  |
| ACPower: 66 |  | -40 |  | dBm |  |
| ACPower: 67 |  | -40 |  | dBm |  |
| ACPower: 68 |  | -40 |  | dBm |  |
| ACPower: 69 |  | -40 |  | dBm |  |
| ACPower: 70 |  | -40 |  | dBm |  |
| ACPower: 71 |  | -40 |  | dBm |  |
| ACPower: 72  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 73 |  | -20 |  | dBm |  |
| ACPower: 74,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 75,  Ptxref |  |  |  | dBm |  |
| ACPower: 76,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 77 |  | -20 |  | dBm |  |
| ACPower: 78,  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 14 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Packet Type: 3-DH5 |  |  |  |  |  |
| Channel : 3,  Exceptions: 2 |  |  |  |  |  |
| ACPower: 0  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 1 |  | -20 |  | dBm |  |
| ACPower: 2,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 3,  Ptxref |  |  |  | dBm |  |
| ACPower: 4,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 5 |  | -20 |  | dBm |  |
| ACPower: 6,  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 7 |  | -40 |  | dBm |  |
| ACPower: 8 |  | -40 |  | dBm |  |
| ACPower: 9 |  | -40 |  | dBm |  |
| ACPower: 10 |  | -40 |  | dBm |  |
| ACPower: 11 |  | -40 |  | dBm |  |
| ACPower: 12 |  | -40 |  | dBm |  |
| ACPower: 13 |  | -40 |  | dBm |  |
| ACPower: 14 |  | -40 |  | dBm |  |
| ACPower: 15 |  | -40 |  | dBm |  |
| ACPower: 16 |  | -40 |  | dBm |  |
| ACPower: 17 |  | -40 |  | dBm |  |
| ACPower: 18 |  | -40 |  | dBm |  |
| ACPower: 19 |  | -40 |  | dBm |  |
| ACPower: 20 |  | -40 |  | dBm |  |
| ACPower: 21 |  | -40 |  | dBm |  |
| ACPower: 22 |  | -40 |  | dBm |  |
| ACPower: 23 |  | -40 |  | dBm |  |
| ACPower: 24 |  | -40 |  | dBm |  |
| ACPower: 25 |  | -40 |  | dBm |  |
| ACPower: 26 |  | -40 |  | dBm |  |
| ACPower: 27 |  | -40 |  | dBm |  |
| ACPower: 28 |  | -40 |  | dBm |  |
| ACPower: 29 |  | -40 |  | dBm |  |
| ACPower: 30 |  | -40 |  | dBm |  |
| ACPower: 31 |  | -40 |  | dBm |  |
| ACPower: 32 |  | -40 |  | dBm |  |
| ACPower: 33 |  | -40 |  | dBm |  |
| ACPower: 34 |  | -40 |  | dBm |  |
| ACPower: 35 |  | -40 |  | dBm |  |
| ACPower: 36 |  | -40 |  | dBm |  |
| ACPower: 37 |  | -40 |  | dBm |  |
| ACPower: 38 |  | -40 |  | dBm |  |
| ACPower: 39 |  | -40 |  | dBm |  |
| ACPower: 40 |  | -40 |  | dBm |  |
| ACPower: 41 |  | -40 |  | dBm |  |
| ACPower: 42 |  | -40 |  | dBm |  |
| ACPower: 43 |  | -40 |  | dBm |  |
| ACPower: 44 |  | -40 |  | dBm |  |
| ACPower: 45 |  | -40 |  | dBm |  |
| ACPower: 46 |  | -40 |  | dBm |  |
| ACPower: 47 |  | -40 |  | dBm |  |
| ACPower: 48 |  | -40 |  | dBm |  |
| ACPower: 49 |  | -40 |  | dBm |  |
| ACPower: 50 |  | -40 |  | dBm |  |
| ACPower: 51 |  | -40 |  | dBm |  |
| ACPower: 52 |  | -40 |  | dBm |  |
| ACPower: 53 |  | -40 |  | dBm |  |
| ACPower: 54 |  | -40 |  | dBm |  |
| ACPower: 55 |  | -40 |  | dBm |  |
| ACPower: 56 |  | -40 |  | dBm |  |
| ACPower: 57 |  | -40 |  | dBm |  |
| ACPower: 58 |  | -40 |  | dBm |  |
| ACPower: 59 |  | -40 |  | dBm |  |
| ACPower: 60 |  | -40 |  | dBm |  |
| ACPower: 61 |  | -40 |  | dBm |  |
| ACPower: 62 |  | -40 |  | dBm |  |
| ACPower: 63 |  | -40 |  | dBm |  |
| ACPower: 64 |  | -40 |  | dBm |  |
| ACPower: 65 |  | -40 |  | dBm |  |
| ACPower: 66 |  | -40 |  | dBm |  |
| ACPower: 67 |  | -40 |  | dBm |  |
| ACPower: 68 |  | -40 |  | dBm |  |
| ACPower: 69 |  | -40 |  | dBm |  |
| ACPower: 70 |  | -40 |  | dBm |  |
| ACPower: 71 |  | -40 |  | dBm |  |
| ACPower: 72 |  | -40 |  | dBm |  |
| ACPower: 73 |  | -40 |  | dBm |  |
| ACPower: 74 |  | -40 |  | dBm |  |
| ACPower: 75 |  | -40 |  | dBm |  |
| ACPower: 76 |  | -40 |  | dBm |  |
| ACPower: 77 |  | -40 |  | dBm |  |
| ACPower: 78 |  | -40 |  | dBm |  |
| Channel : 39,  Exceptions: 2 |  |  |  |  |  |
| ACPower: 0 |  | -40 |  | dBm |  |
| ACPower: 1 |  | -40 |  | dBm |  |
| ACPower: 2 |  | -40 |  | dBm |  |
| ACPower: 3 |  | -40 |  | dBm |  |
| ACPower: 4 |  | -40 |  | dBm |  |
| ACPower: 5 |  | -40 |  | dBm |  |
| ACPower: 6 |  | -40 |  | dBm |  |
| ACPower: 7 |  | -40 |  | dBm |  |
| ACPower: 8 |  | -40 |  | dBm |  |
| ACPower: 9 |  | -40 |  | dBm |  |
| ACPower: 10 |  | -40 |  | dBm |  |
| ACPower: 11 |  | -40 |  | dBm |  |
| ACPower: 12 |  | -40 |  | dBm |  |
| ACPower: 13 |  | -40 |  | dBm |  |
| ACPower: 14 |  | -40 |  | dBm |  |
| ACPower: 15 |  | -40 |  | dBm |  |
| ACPower: 16 |  | -40 |  | dBm |  |
| ACPower: 17 |  | -40 |  | dBm |  |
| ACPower: 18 |  | -40 |  | dBm |  |
| ACPower: 19 |  | -40 |  | dBm |  |
| ACPower: 20 |  | -40 |  | dBm |  |
| ACPower: 21 |  | -40 |  | dBm |  |
| ACPower: 22 |  | -40 |  | dBm |  |
| ACPower: 23 |  | -40 |  | dBm |  |
| ACPower: 24 |  | -40 |  | dBm |  |
| ACPower: 25 |  | -40 |  | dBm |  |
| ACPower: 26 |  | -40 |  | dBm |  |
| ACPower: 27 |  | -40 |  | dBm |  |
| ACPower: 28 |  | -40 |  | dBm |  |
| ACPower: 29 |  | -40 |  | dBm |  |
| ACPower: 30 |  | -40 |  | dBm |  |
| ACPower: 31 |  | -40 |  | dBm |  |
| ACPower: 32 |  | -40 |  | dBm |  |
| ACPower: 33 |  | -40 |  | dBm |  |
| ACPower: 34 |  | -40 |  | dBm |  |
| ACPower: 35 |  | -40 |  | dBm |  |
| ACPower: 36  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 37 |  | -20 |  | dBm |  |
| ACPower: 38,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 39,  Ptxref |  |  |  | dBm |  |
| ACPower: 40,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 41 |  | -20 |  | dBm |  |
| ACPower: 42,  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 43 |  | -40 |  | dBm |  |
| ACPower: 44 |  | -40 |  | dBm |  |
| ACPower: 45 |  | -40 |  | dBm |  |
| ACPower: 46 |  | -40 |  | dBm |  |
| ACPower: 47 |  | -40 |  | dBm |  |
| ACPower: 48 |  | -40 |  | dBm |  |
| ACPower: 49 |  | -40 |  | dBm |  |
| ACPower: 50 |  | -40 |  | dBm |  |
| ACPower: 51 |  | -40 |  | dBm |  |
| ACPower: 52 |  | -40 |  | dBm |  |
| ACPower: 53 |  | -40 |  | dBm |  |
| ACPower: 54 |  | -40 |  | dBm |  |
| ACPower: 55 |  | -40 |  | dBm |  |
| ACPower: 56 |  | -40 |  | dBm |  |
| ACPower: 57 |  | -40 |  | dBm |  |
| ACPower: 58 |  | -40 |  | dBm |  |
| ACPower: 59 |  | -40 |  | dBm |  |
| ACPower: 60 |  | -40 |  | dBm |  |
| ACPower: 61 |  | -40 |  | dBm |  |
| ACPower: 62 |  | -40 |  | dBm |  |
| ACPower: 63 |  | -40 |  | dBm |  |
| ACPower: 64 |  | -40 |  | dBm |  |
| ACPower: 65 |  | -40 |  | dBm |  |
| ACPower: 66 |  | -40 |  | dBm |  |
| ACPower: 67 |  | -40 |  | dBm |  |
| ACPower: 68 |  | -40 |  | dBm |  |
| ACPower: 69 |  | -40 |  | dBm |  |
| ACPower: 70 |  | -40 |  | dBm |  |
| ACPower: 71 |  | -40 |  | dBm |  |
| ACPower: 72 |  | -40 |  | dBm |  |
| ACPower: 73 |  | -40 |  | dBm |  |
| ACPower: 74 |  | -40 |  | dBm |  |
| ACPower: 75 |  | -40 |  | dBm |  |
| ACPower: 76 |  | -40 |  | dBm |  |
| ACPower: 77 |  | -40 |  | dBm |  |
| ACPower: 78 |  | -40 |  | dBm |  |
| Channel : 75,  Exceptions: 2 |  |  |  |  |  |
| ACPower: 0 |  | -40 |  | dBm |  |
| ACPower: 1 |  | -40 |  | dBm |  |
| ACPower: 2 |  | -40 |  | dBm |  |
| ACPower: 3 |  | -40 |  | dBm |  |
| ACPower: 4 |  | -40 |  | dBm |  |
| ACPower: 5 |  | -40 |  | dBm |  |
| ACPower: 6 |  | -40 |  | dBm |  |
| ACPower: 7 |  | -40 |  | dBm |  |
| ACPower: 8 |  | -40 |  | dBm |  |
| ACPower: 9 |  | -40 |  | dBm |  |
| ACPower: 10 |  | -40 |  | dBm |  |
| ACPower: 11 |  | -40 |  | dBm |  |
| ACPower: 12 |  | -40 |  | dBm |  |
| ACPower: 13 |  | -40 |  | dBm |  |
| ACPower: 14 |  | -40 |  | dBm |  |
| ACPower: 15 |  | -40 |  | dBm |  |
| ACPower: 16 |  | -40 |  | dBm |  |
| ACPower: 17 |  | -40 |  | dBm |  |
| ACPower: 18 |  | -40 |  | dBm |  |
| ACPower: 19 |  | -40 |  | dBm |  |
| ACPower: 20 |  | -40 |  | dBm |  |
| ACPower: 21 |  | -40 |  | dBm |  |
| ACPower: 22 |  | -40 |  | dBm |  |
| ACPower: 23 |  | -40 |  | dBm |  |
| ACPower: 24 |  | -40 |  | dBm |  |
| ACPower: 25 |  | -40 |  | dBm |  |
| ACPower: 26 |  | -40 |  | dBm |  |
| ACPower: 27 |  | -40 |  | dBm |  |
| ACPower: 28 |  | -40 |  | dBm |  |
| ACPower: 29 |  | -40 |  | dBm |  |
| ACPower: 30 |  | -40 |  | dBm |  |
| ACPower: 31 |  | -40 |  | dBm |  |
| ACPower: 32 |  | -40 |  | dBm |  |
| ACPower: 33 |  | -40 |  | dBm |  |
| ACPower: 34 |  | -40 |  | dBm |  |
| ACPower: 35 |  | -40 |  | dBm |  |
| ACPower: 36 |  | -40 |  | dBm |  |
| ACPower: 37 |  | -40 |  | dBm |  |
| ACPower: 38 |  | -40 |  | dBm |  |
| ACPower: 39 |  | -40 |  | dBm |  |
| ACPower: 40 |  | -40 |  | dBm |  |
| ACPower: 41 |  | -40 |  | dBm |  |
| ACPower: 42 |  | -40 |  | dBm |  |
| ACPower: 43 |  | -40 |  | dBm |  |
| ACPower: 44 |  | -40 |  | dBm |  |
| ACPower: 45 |  | -40 |  | dBm |  |
| ACPower: 46 |  | -40 |  | dBm |  |
| ACPower: 47 |  | -40 |  | dBm |  |
| ACPower: 48 |  | -40 |  | dBm |  |
| ACPower: 49 |  | -40 |  | dBm |  |
| ACPower: 50 |  | -40 |  | dBm |  |
| ACPower: 51 |  | -40 |  | dBm |  |
| ACPower: 52 |  | -40 |  | dBm |  |
| ACPower: 53 |  | -40 |  | dBm |  |
| ACPower: 54 |  | -40 |  | dBm |  |
| ACPower: 55 |  | -40 |  | dBm |  |
| ACPower: 56 |  | -40 |  | dBm |  |
| ACPower: 57 |  | -40 |  | dBm |  |
| ACPower: 58 |  | -40 |  | dBm |  |
| ACPower: 59 |  | -40 |  | dBm |  |
| ACPower: 60 |  | -40 |  | dBm |  |
| ACPower: 61 |  | -40 |  | dBm |  |
| ACPower: 62 |  | -40 |  | dBm |  |
| ACPower: 63 |  | -40 |  | dBm |  |
| ACPower: 64 |  | -40 |  | dBm |  |
| ACPower: 65 |  | -40 |  | dBm |  |
| ACPower: 66 |  | -40 |  | dBm |  |
| ACPower: 67 |  | -40 |  | dBm |  |
| ACPower: 68 |  | -40 |  | dBm |  |
| ACPower: 69 |  | -40 |  | dBm |  |
| ACPower: 70 |  | -40 |  | dBm |  |
| ACPower: 71 |  | -40 |  | dBm |  |
| ACPower: 72  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |
| ACPower: 73 |  | -20 |  | dBm |  |
| ACPower: 74,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 75,  Ptxref |  |  |  | dBm |  |
| ACPower: 76,  Ptx-26dB |  |  |  | dBm |  |
| ACPower: 77 |  | -20 |  | dBm |  |
| ACPower: 78,  (Exception,limit set to -20dBm) |  | -20 |  | dBm |  |

### RF/TRM/CA/BV-14-C [Enhanced Power Control]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 15 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel:0 |  |  |  |  |  |
| Power at Maximum |  |  |  | dBm |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power at Minimum |  | 4 |  | dBm |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power at Maximum |  |  |  | dBm |  |
| Channel:39 |  |  |  |  |  |
| Power at Maximum |  |  |  | dBm |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power at Minimum |  | 4 |  | dBm |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power at Maximum |  |  |  | dBm |  |
| Channel:78 |  |  |  |  |  |
| Power at Maximum |  |  |  | dBm |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power Step Down | 2 | 8 |  | dB |  |
| Power at Minimum |  | 4 |  | dBm |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power Step Up | 2 | 8 |  | dB |  |
| Power at Maximum |  |  |  | dBm |  |

### RF/RCV/CA/BV-01-C [Sensitivity – single slot packets]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 16 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel: 0 |  | -70 |  | dBm |  |
| Channel: 39 |  | -70 |  | dBm |  |
| Channel: 78 |  | -70 |  | dBm |  |

### RF/RCV/CA/BV-02-C [Sensitivity - multi-slot packets]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 17 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel: 0 |  | -70 |  | dBm |  |
| Channel: 39 |  | -70 |  | dBm |  |
| Channel: 78 |  | -70 |  | dBm |  |

### RF/RCV/CA/BV-03-C [C/I Performance]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 18 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Image Frequency: -2MHz |  |  |  |  |  |
| Channel: 3 |  |  |  |  |  |
| C/I : Co-Channel interference,  BER < 0.1%,  RX Level:-60 |  | 11 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -30 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -9 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -20 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| Channel: 39 |  |  |  |  |  |
| C/I : Co-Channel interference,  BER < 0.1%,  RX Level:-60 |  | 11 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -30 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -9 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -20 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| Channel: 75 |  |  |  |  |  |
| C/I : Co-Channel interference,  BER < 0.1%,  RX Level:-60 |  | 11 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -30 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -9 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -20 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |

### RF/RCV/CA/BV-04-C [Blocking Performance]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 19 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Exceptions Points < 24, Interfering Signal Power Level Test |  |  |  |  |  |
| Interfering Signal Frequency:  30 MHz – 2000 MHz | -10 |  |  | dBm |  |
| Interfering Signal Frequency:  2000 – 2400 MHz | -27 |  |  | dBm |  |
| Interfering Signal Frequency:  2500 – 3000 MHz | -27 |  |  | dBm |  |
| Interfering Signal Frequency:  3000 MHz – 12.75 GHz | -10 |  |  | dBm |  |

### RF/RCV/CA/BV-05-C [Intermodulation Performance]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 20 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| fTX=2f1-f2 and  |f2-f1| = n \* 1 MHz, n=3\4\5, BER < 0.1%, RX Level:-64 |  |  |  |  |  |
| Channel: 0 |  |  |  |  |  |
| Interfering Signal Level | -39 |  |  | dBm |  |
| Channel: 39 |  |  |  |  |  |
| Interfering Signal Level | -39 |  |  | dBm |  |
| Channel: 78 |  |  |  |  |  |
| Interfering Signal Level | -39 |  |  | dBm |  |

### RF/RCV/CA/BV-06-C [Maximum Input Level]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 21 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Max.RX Level, Channel: 0 | -20 |  |  | dBm |  |
| Max.RX Level, Channel: 39 | -20 |  |  | dBm |  |
| Max.RX Level, Channel: 78 | -20 |  |  | dBm |  |

### RF/RCV/CA/BV-07-C [EDR Sensitivity]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 22 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| 2-DH5 |  |  |  |  |  |
| Channel: 0 |  | -70 |  | dBm |  |
| Channel: 39 |  | -70 |  | dBm |  |
| Channel: 78 |  | -70 |  | dBm |  |
| 3-DH5 |  |  |  |  |  |
| Channel: 0 |  | -70 |  | dBm |  |
| Channel: 39 |  | -70 |  | dBm |  |
| Channel: 78 |  | -70 |  | dBm |  |

### RF/RCV/CA/BV-08-C [EDR BER Floor Performance]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 23 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| 2-DH5, RX Level: -60dBm |  |  |  |  |  |
| BER: @ Channel: 0 |  | 0.000007 |  |  |  |
| BER: @ Channel: 39 |  | 0.000007 |  |  |  |
| BER: @ Channel: 78 |  | 0.000007 |  |  |  |
| 3-DH5, RX Level: -60dBm |  |  |  |  |  |
| BER: @ Channel: 0 |  | 0.000007 |  |  |  |
| BER: @ Channel: 39 |  | 0.000007 |  |  |  |
| BER: @ Channel: 78 |  | 0.000007 |  |  |  |

### RF/RCV/CA/BV-09-C [EDR C/I Performance]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 24 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| 2-DH5 |  |  |  |  |  |
| Image Frequency: -2MHz |  |  |  |  |  |
| Channel: 3 |  |  |  |  |  |
| C/I : Co-Channel interference,  BER < 0.1%,  RX Level:-60 |  | 13 | 10 | dB | Pass |
| C/I : Adjacent (+1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 | -28 | dB | Pass |
| C/I : Adjacent (+2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -30 | -35 | dB | Pass |
| C/I : Adjacent (-2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -7 | -30 | dB | Pass |
| C/I : Adjacent (+3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 | -43 | dB | Pass |
| C/I : Adjacent (-3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -20 | -43 | dB | Pass |
| C/I : Adjacent (+4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 | -47 | dB | Pass |
| C/I : Adjacent (-4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 | -47 | dB | Pass |
| Channel: 39 |  |  |  |  |  |
| C/I : Co-Channel interference,  BER < 0.1%,  RX Level:-60 |  | 13 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -30 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -7 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -20 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| Channel: 75 |  |  |  |  |  |
| C/I : Co-Channel interference,  BER < 0.1%,  RX Level:-60 |  | 13 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -30 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -7 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -20 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -40 |  | dB |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 25 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| 3-DH5 |  |  |  |  |  |
| Image Frequency: -2MHz |  |  |  |  |  |
| Channel: 3 |  |  |  |  |  |
| C/I : Co-Channel interference,  BER < 0.1%,  RX Level:-60 |  | 21 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 5 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 5 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -25 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -33 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -13 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -33 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -33 |  | dB |  |
| Channel: 39 |  |  |  |  |  |
| C/I : Co-Channel interference,  BER < 0.1%,  RX Level:-60 |  | 21 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 5 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 5 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -25 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -33 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -13 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -33 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -33 |  | dB |  |
| Channel: 75 |  |  |  |  |  |
| C/I : Co-Channel interference,  BER < 0.1%,  RX Level:-60 |  | 21 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 5 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 5 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | -25 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference,  BER < 0.1%,  RX Level:-60 |  | 0 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -33 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -13 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -33 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference,  BER < 0.1%,  RX Level:-67 |  | -33 |  | dB |  |

### RF/RCV/CA/BV-10-C [EDR Maximum Input Level]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 26 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| 2-DH5 |  |  |  |  |  |
| Max.RX Level, Channel: 0 | -20 |  |  | dBm |  |
| Max.RX Level, Channel: 39 | -20 |  |  | dBm |  |
| Max.RX Level, Channel: 78 | -20 |  |  | dBm |  |
| 3-DH5 |  |  |  |  |  |
| Max.RX Level, Channel: 0 | -20 |  |  | dBm |  |
| Max.RX Level, Channel: 39 | -20 |  |  | dBm |  |
| Max.RX Level, Channel: 78 | -20 |  |  | dBm |  |

# RF BT5 PHY BQB（LE 1M）Test

### RF/TRM-LE/CA/BV-01-C [Output power]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 27 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel:0 |  |  |  |  |  |
| Average Power | -20 | 20 |  | dBm |  |
| Difference  (PowPeak - PowAvg) |  | 3 |  | dB |  |
| Channel:39 |  |  |  |  |  |
| Average Power | -20 | 20 |  | dBm |  |
| Difference  (PowPeak - PowAvg) |  | 3 |  | dB |  |
| Channel:78 |  |  |  |  |  |
| Average Power | -20 | 20 |  | dBm |  |
| Difference  (PowPeak - PowAvg) |  | 3 |  | dB |  |

### RF/TRM-LE/CA/BV-03-C [In-band emissions, uncoded data at 1 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 28 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel:2, Exceptions:0 |  |  |  |  |  |
| In - Band Em.:  2401 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2402 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2403 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2404 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2405 MHz |  |  |  | dBm |  |
| In - Band Em.:  2406 MHz  (center frequency) |  |  |  | dBm |  |
| In - Band Em.:  2407 MHz |  |  |  | dBm |  |
| In - Band Em.:  2408 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2409 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2410 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2411 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2412 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2413 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2414 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2415 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2416 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2417 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2418 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2419 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2420 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2421 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2422 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2423 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2424 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2425 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2426 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2427 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2428 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2429 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2430 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2431 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2432 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2433 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2434 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2435 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2436 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2437 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2438 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2439 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2440 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2441 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2442 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2443 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2444 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2445 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2446 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2447 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2448 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2449 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2450 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2451 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2452 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2453 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2454 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2455 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2456 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2457 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2458 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2459 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2460 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2461 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2462 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2463 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2464 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2465 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2466 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2467 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2468 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2469 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2470 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2471 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2472 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2473 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2474 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2475 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2476 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2477 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2478 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2479 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2480 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2481 MHz |  | -30 |  | dBm |  |
| Channel:19, Exceptions:0 |  |  |  |  |  |
| In - Band Em.:  2401 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2402 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2403 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2404 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2405 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2406 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2407 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2408 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2409 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2410 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2411 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2412 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2413 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2414 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2415 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2416 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2417 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2418 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2419 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2420 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2421 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2422 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2423 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2424 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2425 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2426 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2427 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2428 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2429 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2430 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2431 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2432 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2433 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2434 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2435 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2436 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2437 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2438 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2439 MHz |  |  |  | dBm |  |
| In - Band Em.:  2440 MHz  (center frequency) |  |  |  | dBm |  |
| In - Band Em.:  2441 MHz |  |  |  | dBm |  |
| In - Band Em.:  2442 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2443 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2444 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2445 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2446 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2447 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2448 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2449 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2450 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2451 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2452 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2453 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2454 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2455 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2456 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2457 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2458 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2459 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2460 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2461 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2462 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2463 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2464 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2465 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2466 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2467 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2468 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2469 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2470 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2471 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2472 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2473 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2474 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2475 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2476 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2477 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2478 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2479 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2480 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2481 MHz |  | -30 |  | dBm |  |
| Channel:37, Exceptions:0 |  |  |  |  |  |
| In - Band Em.:  2401 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2402 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2403 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2404 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2405 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2406 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2407 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2408 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2409 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2410 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2411 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2412 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2413 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2414 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2415 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2416 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2417 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2418 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2419 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2420 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2421 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2422 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2423 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2424 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2425 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2426 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2427 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2428 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2429 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2430 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2431 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2432 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2433 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2434 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2435 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2436 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2437 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2438 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2439 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2440 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2441 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2442 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2443 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2444 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2445 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2446 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2447 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2448 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2449 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2450 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2451 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2452 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2453 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2454 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2455 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2456 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2457 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2458 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2459 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2460 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2461 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2462 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2463 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2464 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2465 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2466 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2467 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2468 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2469 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2470 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2471 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2472 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2473 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2474 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2475 MHz |  |  |  | dBm |  |
| In - Band Em.:  2476 MHz  (center frequency) |  |  |  | dBm |  |
| In - Band Em.:  2477 MHz |  |  |  | dBm |  |
| In - Band Em.:  2478 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2479 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2480 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2481 MHz |  | -30 |  | dBm |  |

### RF/TRM-LE/CA/BV-05-C [Modulation Characteristics, uncoded data at 1 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 29 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Delta F1 Avg | 225 | 275 |  | KHz |  |
| Delta F2 99.9% | 185 |  |  | KHz |  |
| Delta F2 Avg / Delta F1 Avg | 0.8 |  |  |  |  |
| Channel : 39 |  |  |  |  |  |
| Delta F1 Avg | 225 | 275 |  | KHz |  |
| Delta F2 99.9% | 185 |  |  | KHz |  |
| Delta F2 Avg / Delta F1 Avg | 0.8 |  |  |  |  |
| Channel : 78 |  |  |  |  |  |
| Delta F1 Avg | 225 | 275 |  | KHz |  |
| Delta F2 99.9% | 185 |  |  | KHz |  |
| Delta F2 Avg / Delta F1 Avg | 0.8 |  |  |  |  |

### RF/TRM-LE/CA/BV-06-C [Carrier frequency offset and drift, uncoded data at 1Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 30 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Frequency Offset | -150 | 150 |  | KHz |  |
| Frequency Drift | -50 | 50 |  | KHz |  |
| Max. Drift Rate (Khz / 50 us) | -20 | 20 |  | KHz |  |
| Initial Frequency Drift | -20 | 20 |  | KHz |  |
| Channel : 19 |  |  |  |  |  |
| Frequency Offset | -150 | 150 |  | KHz |  |
| Frequency Drift | -50 | 50 |  | KHz |  |
| Max. Drift Rate (Khz / 50 us) | -20 | 20 |  | KHz |  |
| Initial Frequency Drift | -20 | 20 |  | KHz |  |
| Channel : 39 |  |  |  |  |  |
| Frequency Offset | -150 | 150 |  | KHz |  |
| Frequency Drift | -50 | 50 |  | KHz |  |
| Max. Drift Rate (Khz / 50 us) | -20 | 20 |  | KHz |  |
| Initial Frequency Drift | -20 | 20 |  | KHz |  |

### RF/RCV-LE/CA/BV-01-C [Receiver sensitivity, uncoded data at 1 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 31 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel: 0 |  | -70 |  | dBm |  |
| Channel: 19 |  | -70 |  | dBm |  |
| Channel: 39 |  | -70 |  | dBm |  |

### RF/RCV-LE/CA/BV-03-C [C/I and Receiver Selectivity Performance, uncoded data at 1 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 32 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Image Frequency: -2MHz,  PER < 30.8%,  RX Level:-67 |  |  |  |  |  |
| Channel: 2 |  |  |  |  |  |
| C/I : Co-Channel interferenc |  | 21 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference |  | 15 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference |  | 15 |  | dB |  |
| C/I : Adjacent (+2 MHz) interferenc |  | -17 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference |  | -9 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference |  | -15 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference |  | -27 |  | dB |  |
| Channel: 19 |  |  |  |  |  |
| C/I : Co-Channel interferenc |  | 21 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference |  | 15 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference |  | 15 |  | dB |  |
| C/I : Adjacent (+2 MHz) interferenc |  | -17 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference |  | -9 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference |  | -15 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference |  | -27 |  | dB |  |
| Channel: 37 |  |  |  |  |  |
| C/I : Co-Channel interferenc |  | 21 |  | dB |  |
| C/I : Adjacent (+1 MHz) interference |  | 15 |  | dB |  |
| C/I : Adjacent (-1 MHz) interference |  | 15 |  | dB |  |
| C/I : Adjacent (+2 MHz) interferenc |  | -17 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference |  | -9 |  | dB |  |
| C/I : Adjacent (+3 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-3 MHz) interference |  | -15 |  | dB |  |
| C/I : Adjacent (+4 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference |  | -27 |  | dB |  |

### RF/RCV-LE/CA/BV-04-C [Blocking Performance, uncoded data at 1 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 33 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Exceptions Points < 10, Interfering Signal Power Level Test |  |  |  |  |  |
| Interfering Signal Frequency:  30 MHz – 2000 MHz | -30 |  |  | dBm |  |
| Interfering Signal Frequency:  2000 – 2400 MHz | -35 |  |  | dBm |  |
| Interfering Signal Frequency:  2500 – 3000 MHz | -35 |  |  | dBm |  |
| Interfering Signal Frequency:  3000 MHz – 12.75 GHz | -30 |  |  | dBm |  |

### RF/RCV-LE/CA/BV-05-C [Intermodulation Performance, uncoded data at 1 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 34 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| fTX=2f1-f2 and  |f2-f1| = n \* 1 MHz, n=3\4\5, BER < 0.1%, RX Level:-64 |  |  |  |  |  |
| Channel: 0 |  |  |  |  |  |
| Interfering Signal Level | -50 |  |  | dBm |  |
| Channel: 19 |  |  |  |  |  |
| Interfering Signal Level | -50 |  |  | dBm |  |
| Channel: 39 |  |  |  |  |  |
| Interfering Signal Level | -50 |  |  | dBm |  |

### RF/RCV-LE/CA/BV-06-C [Maximum input signal level, uncoded data at 1 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 35 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Max.RX Level, Channel: 0 | -10 |  |  | dBm |  |
| Max.RX Level, Channel: 19 | -10 |  |  | dBm |  |
| Max.RX Level, Channel: 39 | -10 |  |  | dBm |  |

### RF/RCV-LE/CA/BV-07-C [PER Report Integrity, uncoded data at 1 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 36 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| RX Level: -30 dBm |  |  |  |  |  |
| PER @ Channel: 0 | 50 | 65.4 |  | % |  |
| PER @ Channel: 19 | 50 | 65.4 |  | % |  |
| PER @ Channel: 39 | 50 | 65.4 |  | % |  |

# RF BT5 PHY BQB（LE 2M）Test

### RF/TRM-LE2M/CA/BV-01-C [Output power]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 37 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel:0 |  |  |  |  |  |
| Average Power | -20 | 20 |  | dBm |  |
| Difference  (PowPeak - PowAvg) |  | 3 |  | dB |  |
| Channel:39 |  |  |  |  |  |
| Average Power | -20 | 20 |  | dBm |  |
| Difference  (PowPeak - PowAvg) |  | 3 |  | dB |  |
| Channel:78 |  |  |  |  |  |
| Average Power | -20 | 20 |  | dBm |  |
| Difference  (PowPeak - PowAvg) |  | 3 |  | dB |  |

### RF/TRM-LE2M/CA/BV-03-C [In-band emissions, uncoded data at 2 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 38 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel:2, Exceptions:0 |  |  |  |  |  |
| In - Band Em.:  2401 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2402 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2403 MHz |  |  |  | dBm |  |
| In - Band Em.:  2404 MHz |  |  |  | dBm |  |
| In - Band Em.:  2405 MHz |  |  |  | dBm |  |
| In - Band Em.:  2406 MHz  (center frequency) |  |  |  | dBm |  |
| In - Band Em.:  2407 MHz |  |  |  | dBm |  |
| In - Band Em.:  2408 MHz |  |  |  | dBm |  |
| In - Band Em.:  2409 MHz |  |  |  | dBm |  |
| In - Band Em.:  2410 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2411 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2412 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2413 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2414 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2415 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2416 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2417 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2418 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2419 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2420 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2421 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2422 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2423 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2424 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2425 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2426 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2427 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2428 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2429 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2430 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2431 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2432 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2433 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2434 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2435 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2436 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2437 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2438 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2439 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2440 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2441 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2442 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2443 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2444 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2445 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2446 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2447 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2448 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2449 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2450 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2451 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2452 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2453 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2454 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2455 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2456 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2457 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2458 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2459 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2460 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2461 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2462 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2463 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2464 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2465 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2466 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2467 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2468 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2469 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2470 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2471 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2472 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2473 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2474 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2475 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2476 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2477 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2478 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2479 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2480 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2481 MHz |  | -30 |  | dBm |  |
| Channel:19, Exceptions:0 |  |  |  |  |  |
| In - Band Em.:  2401 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2402 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2403 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2404 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2405 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2406 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2407 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2408 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2409 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2410 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2411 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2412 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2413 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2414 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2415 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2416 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2417 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2418 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2419 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2420 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2421 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2422 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2423 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2424 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2425 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2426 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2427 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2428 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2429 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2430 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2431 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2432 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2433 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2434 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2435 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2436 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2437 MHz |  |  |  | dBm |  |
| In - Band Em.:  2438 MHz |  |  |  | dBm |  |
| In - Band Em.:  2439 MHz |  |  |  | dBm |  |
| In - Band Em.:  2440 MHz  (center frequency) |  |  |  | dBm |  |
| In - Band Em.:  2441 MHz |  |  |  | dBm |  |
| In - Band Em.:  2442 MHz |  |  |  | dBm |  |
| In - Band Em.:  2443 MHz |  |  |  | dBm |  |
| In - Band Em.:  2444 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2445 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2446 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2447 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2448 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2449 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2450 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2451 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2452 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2453 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2454 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2455 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2456 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2457 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2458 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2459 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2460 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2461 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2462 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2463 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2464 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2465 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2466 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2467 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2468 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2469 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2470 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2471 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2472 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2473 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2474 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2475 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2476 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2477 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2478 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2479 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2480 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2481 MHz |  | -30 |  | dBm |  |
| Channel:37, Exceptions:0 |  |  |  |  |  |
| In - Band Em.:  2401 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2402 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2403 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2404 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2405 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2406 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2407 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2408 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2409 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2410 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2411 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2412 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2413 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2414 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2415 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2416 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2417 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2418 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2419 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2420 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2421 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2422 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2423 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2424 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2425 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2426 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2427 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2428 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2429 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2430 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2431 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2432 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2433 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2434 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2435 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2436 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2437 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2438 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2439 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2440 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2441 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2442 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2443 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2444 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2445 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2446 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2447 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2448 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2449 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2450 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2451 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2452 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2453 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2454 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2455 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2456 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2457 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2458 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2459 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2460 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2461 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2462 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2463 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2464 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2465 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2466 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2467 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2468 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2469 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2470 MHz |  | -30 |  | dBm |  |
| In - Band Em.:  2471 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2472 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2473 MHz |  |  |  | dBm |  |
| In - Band Em.:  2474 MHz |  |  |  | dBm |  |
| In - Band Em.:  2475 MHz |  |  |  | dBm |  |
| In - Band Em.:  2476 MHz  (center frequency) |  |  |  | dBm |  |
| In - Band Em.:  2477 MHz |  |  |  | dBm |  |
| In - Band Em.:  2478 MHz |  |  |  | dBm |  |
| In - Band Em.:  2479 MHz |  |  |  | dBm |  |
| In - Band Em.:  2480 MHz |  | -20 |  | dBm |  |
| In - Band Em.:  2481 MHz |  | -20 |  | dBm |  |

### RF/TRM-LE2M/CA/BV-05-C [Modulation Characteristics, uncoded data at 2 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 39 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Delta F1 Avg | 450 | 550 |  | KHz |  |
| Delta F2 99.9% | 370 |  |  | KHz |  |
| Delta F2 Avg / Delta F1 Avg | 0.8 |  |  |  |  |
| Channel : 39 |  |  |  |  |  |
| Delta F1 Avg | 450 | 550 |  | KHz |  |
| Delta F2 99.9% | 370 |  |  | KHz |  |
| Delta F2 Avg / Delta F1 Avg | 0.8 |  |  |  |  |
| Channel : 78 |  |  |  |  |  |
| Delta F1 Avg | 450 | 550 |  | KHz |  |
| Delta F2 99.9% | 370 |  |  | KHz |  |
| Delta F2 Avg / Delta F1 Avg | 0.8 |  |  |  |  |

### RF/TRM-LE2M/CA/BV-06-C [Carrier frequency offset and drift, uncoded data at 2Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 40 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel : 0 |  |  |  |  |  |
| Frequency Offset | -150 | 150 |  | KHz |  |
| Frequency Drift | -50 | 50 |  | KHz |  |
| Max. Drift Rate (Khz / 50 us) | -20 | 20 |  | KHz |  |
| Initial Frequency Drift | -20 | 20 |  | KHz |  |
| Channel : 19 |  |  |  |  |  |
| Frequency Offset | -150 | 150 |  | KHz |  |
| Frequency Drift | -50 | 50 |  | KHz |  |
| Max. Drift Rate (Khz / 50 us) | -20 | 20 |  | KHz |  |
| Initial Frequency Drift | -20 | 20 |  | KHz |  |
| Channel : 39 |  |  |  |  |  |
| Frequency Offset | -150 | 150 |  | KHz |  |
| Frequency Drift | -50 | 50 |  | KHz |  |
| Max. Drift Rate (Khz / 50 us) | -20 | 20 |  | KHz |  |
| Initial Frequency Drift | -20 | 20 |  | KHz |  |

### RF/RCV-LE2M/CA/BV-01-C [Receiver sensitivity, uncoded data at 2 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 41 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Channel: 0 |  | -70 |  | dBm |  |
| Channel: 19 |  | -70 |  | dBm |  |
| Channel: 39 |  | -70 |  | dBm |  |

### RF/RCV-LE2M/CA/BV-03-C [C/I and Receiver Selectivity Performance, uncoded data at 2 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 42 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Image Frequency: -2MHz,  PER < 30.8%,  RX Level:-67 |  |  |  |  |  |
| Channel: 2 |  |  |  |  |  |
| C/I : Co-Channel interferenc |  | 21 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference |  | 15 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference |  | -9 |  | dB |  |
| C/I : Adjacent (+4 MHz) interferenc |  | -17 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference |  | -15 |  | dB |  |
| C/I : Adjacent (+6 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-6 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (+8 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-8 MHz) interference |  | -27 |  | dB |  |
| Channel: 19 |  |  |  |  |  |
| C/I : Co-Channel interferenc |  | 21 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference |  | 15 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference |  | -9 |  | dB |  |
| C/I : Adjacent (+4 MHz) interferenc |  | -17 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference |  | -15 |  | dB |  |
| C/I : Adjacent (+6 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-6 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (+8 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-8 MHz) interference |  | -27 |  | dB |  |
| Channel: 37 |  |  |  |  |  |
| C/I : Co-Channel interferenc |  | 21 |  | dB |  |
| C/I : Adjacent (+2 MHz) interference |  | 15 |  | dB |  |
| C/I : Adjacent (-2 MHz) interference |  | -9 |  | dB |  |
| C/I : Adjacent (+4 MHz) interferenc |  | -17 |  | dB |  |
| C/I : Adjacent (-4 MHz) interference |  | -15 |  | dB |  |
| C/I : Adjacent (+6 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-6 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (+8 MHz) interference |  | -27 |  | dB |  |
| C/I : Adjacent (-8 MHz) interference |  | -27 |  | dB |  |

### RF/RCV-LE2M/CA/BV-04-C [Blocking Performance, uncoded data at 2 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 43 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Exceptions Points < 10, Interfering Signal Power Level Test |  |  |  |  |  |
| Interfering Signal Frequency:  30 MHz – 2000 MHz | -30 |  |  | dBm |  |
| Interfering Signal Frequency:  2000 – 2400 MHz | -35 |  |  | dBm |  |
| Interfering Signal Frequency:  2500 – 3000 MHz | -35 |  |  | dBm |  |
| Interfering Signal Frequency:  3000 MHz – 12.75 GHz | -30 |  |  | dBm |  |

### RF/RCV-LE2M/CA/BV-05-C [Intermodulation Performance, uncoded data at 2 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 44 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| fTX=2f1-f2 and  |f2-f1| = n \* 2 MHz, n=3\4\5, BER < 0.1%, RX Level:-64 |  |  |  |  |  |
| Channel: 0 |  |  |  |  |  |
| Interfering Signal Level | -50 |  |  | dBm |  |
| Channel: 19 |  |  |  |  |  |
| Interfering Signal Level | -50 |  |  | dBm |  |
| Channel: 39 |  |  |  |  |  |
| Interfering Signal Level | -50 |  |  | dBm |  |

### RF/RCV-LE2M/CA/BV-06-C [Maximum input signal level, uncoded data at 2 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 45 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| Max.RX Level, Channel: 0 | -10 |  |  | dBm |  |
| Max.RX Level, Channel: 19 | -10 |  |  | dBm |  |
| Max.RX Level, Channel: 39 | -10 |  |  | dBm |  |

### RF/RCV-LE2M/CA/BV-07-C [PER Report Integrity, uncoded data at 2 Ms/s]

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Table 46 | | | | | |
| Test Name and Condition | Low Limit | Upper Limit | Measure Value | Unit | Pass/Fail |
| RX Level: -30 dBm |  |  |  |  |  |
| PER @ Channel: 0 | 50 | 65.4 |  | % |  |
| PER @ Channel: 19 | 50 | 65.4 |  | % |  |
| PER @ Channel: 39 | 50 | 65.4 |  | % |  |